FieldPoint / Real-Time Test Results

An FP-TC-120 module was used in conjunction with each controller to do all the tests.  The tests were done on a machine that had LabVIEW 7.0 and FieldPoint 4.0.1 installed.  I wasn’t able to install version 4.1 in the computer, since the installer refuses to load on a 64-bit system.
 
FP-1000
+ Able to find in MAX using the highest baud rate (115200).  I did not test using a slower baud rate.
+ Could configure the TC-120, and read the right values from MAX.
+ Could read from LabVIEW 7.0 using a FieldPoint Express VI.

FP-1601
+ Able to find in MAX, to assign IP Address and do all the configuration for the controller and the TC module.
+ Read and Write from MAX.
+ Successful set a snapshot for the controller.
+ Watchdog for the controller is working as well.
+ Using the FieldPoint Express VI, reading and writing from the controller and the TC module worked fine.  There was no difference in speed when reading and writing using LabVIEW.

FP-2000
+ Able to find in MAX, to assign IP Address and do all the configuration for the controller and the TC module.
+ Read and Write from MAX.
+ Successfully set a snapshot for the controller.
+ Successfully set the power-up state for the LEDs of the controller.
+ Watchdog for the controller is working as well.
+ Using the FieldPoint Express VI, reading and writing from the controller and the TC module worked fine.  There was no difference in speed when reading and writing using LabVIEW.
+ RT was installed successfully and the RT software installed on the FP controller with no problems at all.
+ RT Communication Wizard:
-	Worked fine for the 4 different forms of communication:  TCP/IP, UDP, DataSocket, and Logos.

+ Developing an application and embedding that as a startup executable worked.
+ The web server appears work correctly.